**Earthing wall collar**

for round and flat conductors

Article Code: HMK

GTIN: -

Brand: Hauff-Technik

Water barrier flange for water pressure-tight integration of earth conductors in floor slabs or concrete walls.

Material: Water barrier flange: EPDM; Clamping straps: W1

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de