**Closed sealing element set**

for multi-line building entry systems

Article Code: SDS2 E/W/K

GTIN: -

Brand: Hauff-Technik

Dimensions: Area of application SDE: 1 Electric cable with Øa 26-29, 36-39, 43-46 or 48-51 mm; Area of application SDW: 1 water line OD 32, 40 or 50 mm; Area of application SDK: 1 cable OD 13 - 21 mm, 3 cables OD 7 - 13 mm, 1 cable OD 5 - 13 mm

Material: Sealing elements: glass fibre reinforced polyamide/EPDM

Features: with segments for maximum area of application

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de