**corrugated pipe set**

For entry into the pylon marker

Article Code: 2LINE G-BOX WR SET

GTIN: -

Brand: Hauff-Technik

For protected installation of the 2-LINE G-BOX cable system or a fiber optic cable up to the pylons. Features: Length 0.75 m, clip on both sides for connection to the 2LINE G-BOX, sealing grommet on one side.

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de