**Foil sleeve**

for entries through the floor slab

Article Code: HFM

GTIN: -

Brand: Hauff-Technik

Hauff foil sleeve for the safe connection of penetrations through the floor slab to a vapour barrier foil, radon foil or other sheet-like sealing on the floor slab.

Material: Foil flange: Aluminium-plastic composite foil with butyl rubber; Rubber insert: EPDM

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight; radon-proof

Features: Easy integration of the vapour barrier or radon foil; Prevents convection and therefore the penetration of radon gas into the building

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de