**ETGAR insert for building services outlet**

for buildings without a basement

Article Code: HAB ETGAR EBT

GTIN: -

Brand: Hauff-Technik

For routing and distributing electric power and communication lines from the building to the surrounding property. Is supplemented with empty conduit system, seal insert and sealing elements.

Material: Wall sleeve: ABS; Installation fixture: St37

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

Features: variable height adaptation to the finished floor level

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de