**Sealing element**

for ETGAR building services outlet

Article Code: HAB ETGAR DB 1x13-21+3x7-13+1x5-13

GTIN: -

Brand: Hauff-Technik

For mounting in ETGAR building services outlet and for sealing lines. With segments for maximum area of application.

Dimensions: Area of application: 1 cable OD 13 - 21 mm, 3 cables OD 7 - 13 mm, 1 cable OD 5 - 13 mm

Material: Sleeve caps: EPDM; Clamping straps: stainless steel V2A (AISI 304L); Pipe: PVC-U

Features: with segments for maximum area of application

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de