**Corrugated pipe**

for ETGAR extension set

Article Code: WR32 GU25000

GTIN: -

Brand: Hauff-Technik

Empty conduit system for further distributing cables to the property and to connect to the 2LINE G-BOX ETGAR extension set.

Dimensions: Øb: 24 mm; Øa: 32 mm

Material: PE

Tightness: gastight and watertight

Features: high degree of flexibility thanks to narrow radii

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de