**Eexcess length box**

for installation on the customer's property

Article Code: 2LINE G-BOX UEB

GTIN: -

Brand: Hauff-Technik

Features: 1 entry pot with cover including fastening material for attaching the corrugated conduit to the cable overlength box. Set includes all parts required for connection to the 2LINE G-BOX for protected laying of the fiber optic cable to the customer building.

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de