**Pipe connection sleeve**

Material: Sleeve: EPDM; Clamping straps: stainless steel V2A (AISI 304L)

Tightness: gastight and watertight to 2.5 bar

Features: gastight and watertight sleeve method also suitable for built-over applications

Article Code: KES110 MA110-125/90-113

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de